**STANDARD SPECIFICATIONS**

* Single function shower head



* 2.5gpm flow rate
* 8” round shower head
* 14” long arm

**FINISHES INCLUDE**

* Chrome (UF91000)
* Brushed nickel (UF91003)

**WARRANTY**

* Limited lifetime warranty on workmanship and materials to the original purchaser

**COMPLIES WITH**

* ANSI/ASME A112.18.1
* CSA B125-1
* IAPMO/UPC/CUPC

